Pittsfield Village Condominium Association

Gas Fireplace Specifications

•	Must be a direct-vent natural gas fireplace, not a 'ventless'
•	Unit must be vented to exterior of unit.
•	All work must be completed by a licensed mechanical contractor.
•	A building permit copy must be submitted to office before commencement of work.
•	Exterior vent must have a termination cap that is 'Cool to the Touch' and not in plain view from street. 
•	Termination Cap must be painted to match building color.
•	Termination Cap must adhere to the following clearances:
12" above grade or deck
12" to operable window or door
9" to outside corner

If you have any questions, contact the Pittsfield Village Maintenance Supervisor at (734 971-0233).